{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"merged":[[0,0,0,5],[2,2,7,2],[30,0,31,0],[30,1,31,1],[30,3,31,3],[30,4,31,4],[30,5,31,5]]}
["山东航空学院工会教工活动室工程量清单"]
["序号","项目名称","施工工艺及施工做法","单位","工程量","备注"]
[1,"普通铝型材门拆除","人工及机械拆除，垃圾负责外运学校","套",1]
[2,"蓝色隔断拆除",null,"项",1]
[3,"铝塑板吊顶、包柱拆除",null,"㎡",60]
[4,"地面地胶拆除",null,"㎡",276]
[5,"顶面老旧灯具拆除",null,"项",1]
[6,"场地清理",null,"㎡",276]
[7,"入口大门","2.0厚度断桥铝肯德基定做安装","㎡",3.5]
[8,"窗帘","1500*1500 5个;1700*1500 5个;浅灰;半遮光卷帘定制+安装","组",10]
[9,"入口钢架焊接造型骨架","40*60*3mm镀锌方管焊接骨架，方管间距不大于1000mm","㎡",24]
[10,"轻钢石膏板隔墙","75型轻钢龙骨骨架，双面单层石膏板面层，中间填充岩棉","㎡",70]
[11,"入口形象墙木饰面","基层清理，定制厚度不低于6mm木纹饰面板，结构胶固定于指定部位","㎡",22]
[12,"管理室门+套","实木复合烤漆套装平开门定制安装","套",1]
[13,"更衣室门+套","实木复合烤漆套装平开门定制安装","套",2]
[14,"储藏室隐形门","75型轻钢龙骨加固处理，40mm平板门制作安装，含五金件","项",1]
[15,"墙面单色乳胶漆","抹面石膏局部找补，防碱腻子基础找平两遍，精细打磨，滚涂乳胶漆2遍","㎡",200]
[16,"入口墙面造型拼色乳胶漆","抹面石膏局部找补，防碱腻子基础找平两遍，精细打磨，滚涂乳胶漆2遍，拼色部分纸胶带防护滚涂指定颜色乳胶漆3遍","㎡",48]
[17,"立柱拼色乳胶漆","抹面石膏局部找补，防碱腻子基础找平两遍，精细打磨，滚涂乳胶漆2遍，拼色部分纸胶带防护滚涂指定颜色乳胶漆3遍","㎡",36]
[18,"暖气管线翻新","管线面层清理，打磨生锈部分，滚涂银粉饰面","项",1]
[19,"顶面造型吊顶修复","面层清理，修复脱落开胶顶面铝塑板","项",1]
[20,"木饰面造型吊顶","Φ8吊筋顶面固定，轻钢C50主龙骨，c50副龙骨，9.5石膏板做造型制作基础，面层粘贴指定颜色木饰面","㎡",32]
[21,"铝方通吊顶","钢架造型基础上专用吊顶龙骨制作基础，卡50*60mm白色铝方通","㎡",36]
[22,"入口悬空双面石膏板吊顶","木工板制作上面基础，下面轻钢C50主龙骨，c50副龙骨制作基础面层，双层石膏板饰面","㎡",13]
[23,"塑胶地板","基础清理，自流平水泥找平，面层粘贴6mm运动塑胶","㎡",217]
[24,"木地板","基础清理，快干粉局部找平，防潮垫满铺，面层铺贴指定颜色木地板饰面","㎡",60]
[25,"地面金属压条","定制木地板专用平板金属压条","m",15]
[26,"强电线路敷设","线路为绿灯行电线、线管为联塑pvc","㎡",276]
[27,"吊装长条灯","品牌：木林森、三雄极光、佛山照明","盏",10,"24W 6500K 1200*80*60直角哑黑"]
[28,"铝方通双头筒灯","品牌：木林森、三雄极光、佛山照明","盏",8,"双头2*6W【暖白4000K】开孔9*16cm"]
[29,"开关、五孔面板","品牌：三雄极光、公牛、飞利浦","项",1]
[null,null,"3C认证 10A250V二三极宽体插座开关"]
[30,"墙面广告画面及雕刻字制作及安装","墙面pvc画面及雕刻字制作","项",1]
[31,"隔断架","1400*3000","项",1]